Update History
MOSIS AMI 0.5um - Submicron Rules
**************************************
08Oct2001
- Updated Technology name to SCN3ME_SUBM, was SCN3M_SUBM.
- Updated all large metal rules to ignore all condition in DRC setup.
- Updated SPR setup (31Oct2001)

30July2001
- Update with current Mosis rules for AMI C5N SCN3ME

29Dec2000
- Poly2 width for cap is updated to 7 lambda.

31Jan2000
- Added rule 27.6b
- Removed NW/Poly resistor

17Jan2000
-mAMIs05.tdb, mAMIs05DL.tdb: updated poly2 wire to include: not "High Res Implant"
                      
05Oct99
-mAMIs05.tdb: 	DRC rules 8.5 (a,b,c,d) are disabled
		DRC rules 9.2 (b,c) are disabled
-mAMIs05.ext:	Add statement for poly resistor over Nwell
 
Initial Released 03SEP99
- MOSIS AMI 0.5um Design Kit
  Technology = SCN3M_SUBM lambda = 0.30um

**************************************                         
Copyright (c) 2001 Tanner Research, Inc.  All rights reserved.

Tanner Research, Inc.
2650 East Foothill Blvd.
Pasadena, CA  91107 USA

Telephone: (626) 792-3000
Fax:       (626) 792-0300
e-mail:    ces@tanner.com
