                                          
                           MOSIS PARAMETRIC TEST RESULTS
                                          
            RUN: T2AH                                        VENDOR: AMI
     TECHNOLOGY: SCN15                                FEATURE SIZE: 1.6 microns


INTRODUCTION: This report contains the lot average results obtained by MOSIS
              from measurements of MOSIS test structures on each wafer of
              this fabrication lot. SPICE parameters obtained from similar
              measurements on a selected wafer are also attached.

COMMENTS: American Microsystems, Inc. 1.5 micron AB(X)


TRANSISTOR PARAMETERS   W/L      N-CHANNEL P-CHANNEL  UNITS
                                                     
 MINIMUM                4.0/1.6                      
  Vth                                 0.57     -0.97  volts
                                                     
 SHORT                  20.0/1.6                     
  Idss                              176       -67     uA/um
  Vth                                 0.54     -0.92  volts
  Vpt                                10.0     -10.0   volts
                                                     
 WIDE                   20.0/1.6                     
  Ids0                              < 2.5     < 2.5   pA/um
                                                     
 LARGE                  50/50                        
  Vth                                 0.57     -0.88  volts
  Vjbkd                              16.6     -14.6   volts
  Ijlk                              <50.0     <50.0   pA
  Gamma                               0.58      0.49  V^0.5
                                                     
 K' (Uo*Cox/2)                       35.3     -11.6   uA/V^2
 Low-field Mobility                 652.22    214.33  cm^2/V*s

                                                     
COMMENTS: Poly bias varies with design technology. To account for mask and
           etch bias use the appropriate value for the parameter XL in your
           SPICE model card.
                       Design Technology                   XL
                       -----------------                   -------
                       SCN (lambda=0.6)                     0.00
                       SCN (lambda=0.8)                     0.00
                       AMI_ABN                              0.00


POLY2 TRANSISTORS       W/L      N-CHANNEL P-CHANNEL  UNITS
                                                     
 MINIMUM                4.8/3.2                      
  Vth                                 0.91     -1.10  volts
                                                     
 SHORT                  9.6/3.2                      
  Vth                                 0.89     -1.06  volts
                                                     
 LARGE                  28.8/28.                     
  Vth                                 0.90     -1.05  volts
                                                     
 K' (Uo*Cox/2)                       21.7      -7.1   uA/V^2
                                                     



FOX TRANSISTORS         GATE      N+ACTIVE  P+ACTIVE  UNITS
 Vth                    Poly        >15.0    <-15.0   volts



BIPOLAR PARAMETERS      W/L          NPN              UNITS

 2X1                    2X1
  Beta                              124
  V_early                            45.8             volts
  Vce,sat                             0.2             volts

 2X2                    2X2
  Beta                              124
  V_early                            45.8             volts
  Vce,sat                             ---             volts

 2X4                    2X4
  Beta                              124
  V_early                            45.6             volts
  Vce,sat                             ---             volts

 2X8                    2X8
  Beta                              125
  V_early                            45.2             volts
  Vce,sat                             ---             volts
  BVceo                              12.0             volts
  BVcbo                              29.0             volts
  BVebo                               7.9             volts



PROCESS PARAMETERS    N+ACTV P+ACTV  POLY  POLY2  PBASE    MTL1  MTL2  UNITS
 Sheet Resistance      52.7   76.0  28.5   24.1    2216.8  0.05  0.03  ohms/sq
 Contact Resistance    50.4   42.4  41.5   16.7                  0.05  ohms
 Gate Oxide Thickness 319                                              angstrom

PROCESS PARAMETERS       N_WELL   UNITS
 Sheet Resistance        1658     ohms/sq
 Contact Resistance               ohms




CAPACITANCE PARAMETERS  N+ACTV  P+ACTV   POLY  POLY2  M1  M2   N_WELL   UNITS
 Area (substrate)       269     299       36          24  14     60     aF/um^2
 Area (N+active)                        1083   691    49  25            aF/um^2
 Area (P+active)                        1066   684                      aF/um^2
 Area (poly)                                   561    44  22            aF/um^2
 Area (poly2)                                         45                aF/um^2
 Area (metal1)                                            36            aF/um^2
 Fringe (substrate)      98     159                   32  37            aF/um
 Fringe (poly)                                        58  43            aF/um
 Fringe (metal1)                                          53            aF/um
 Overlap (N+active)                      172                            aF/um
 Overlap (P+active)                      213                            aF/um
                                                              


CIRCUIT PARAMETERS                          UNITS      
 Inverters                   K                         
  Vinv                      1.0       1.78  volts      
  Vinv                      1.5       2.10  volts      
  Vol (100 uA)              2.0       0.31  volts      
  Voh (100 uA)              2.0       4.53  volts      
  Vinv                      2.0       2.31  volts      
  Gain                      2.0     -15.46             
 Ring Oscillator Freq.                                 
  DIV64 (31-stg,5.0V)                36.11  MHz        
 Ring Oscillator Power                                 
  DIV64 (31-stg,5.0V)                 1.53  uW/MHz/gate
                                                       

 T2AH SPICE LEVEL3 PARAMETERS

*
* DATE: Dec  3/02                                                               
* LOT: t2ah                  WAF: 7203                                          
* DIE: N_Area_Fring          DEV: 20.00/20.0                                    
* Temp= 27                                                                      
.MODEL CMOSN NMOS (                                 LEVEL  = 3                  
+ TOX    = 3.19E-8         NSUB   = 3.984897E15     GAMMA  = 0.7093689          
+ PHI    = 0.7             VTO    = 0.5972338       DELTA  = 0.4276796          
+ UO     = 629.8251141     ETA    = 1.119853E-3     THETA  = 0.0715349          
+ KP     = 6.89818E-5      VMAX   = 2.29286E5       KAPPA  = 0.5                
+ RSH    = 0.0431787       NFS    = 5.226795E11     TPG    = 1                  
+ XJ     = 3E-7            LD     = 0               WD     = 7.018097E-7        
+ CGDO   = 1.72E-10        CGSO   = 1.72E-10        CGBO   = 1E-10              
+ CJ     = 2.703221E-4     PB     = 0.7170386       MJ     = 0.5                
+ CJSW   = 1.355051E-10    MJSW   = 0.0499995       )                           
*                                                                               
*                                                                               
* DATE: Dec  3/02                                                               
* LOT: T2AH                  WAF: 7203                                          
* DIE: P_Area_Fring          DEV: P3740/10                                      
* Temp= 27                                                                      
.MODEL CMOSP PMOS (                                 LEVEL  = 3                  
+ TOX    = 3.19E-8         NSUB   = 1E17            GAMMA  = 0.5098214          
+ PHI    = 0.7             VTO    = -0.8893383      DELTA  = 0.4065392          
+ UO     = 102.9115558     ETA    = 9.842906E-6     THETA  = 0.1300665          
+ KP     = 2.317741E-5     VMAX   = 3.414958E5      KAPPA  = 150                
+ RSH    = 37.9509969      NFS    = 4.059505E11     TPG    = -1                 
+ XJ     = 2E-7            LD     = 1E-14           WD     = 1E-6               
+ CGDO   = 2.13E-10        CGSO   = 2.13E-10        CGBO   = 1E-10              
+ CJ     = 3.003062E-4     PB     = 0.7373286       MJ     = 0.4287192          
+ CJSW   = 1.637795E-10    MJSW   = 0.1005589       )                           
*                                                                               

 T2AH SPICE BSIM3 VERSION 3.1 PARAMETERS

SPICE 3f5 Level 8, Star-HSPICE Level 49, UTMOST Level 8

* DATE: Dec  3/02
* LOT: T2AH                  WAF: 7203
* Temperature_parameters=Default
.MODEL CMOSN NMOS (                                LEVEL   = 49
+VERSION = 3.1            TNOM    = 27             TOX     = 3.19E-8
+XJ      = 3E-7           NCH     = 7.5E16         VTH0    = 0.5449692
+K1      = 0.9382683      K2      = -0.0814687     K3      = 4.9971343
+K3B     = -1.205599      W0      = 1E-7           NLX     = 1E-8
+DVT0W   = 0              DVT1W   = 0              DVT2W   = 0
+DVT0    = 0.5628191      DVT1    = 0.2776207      DVT2    = -0.3521233
+U0      = 670.5086073    UA      = 1.96216E-9     UB      = 1.294827E-18
+UC      = 4.099991E-11   VSAT    = 1.104603E5     A0      = 0.5815491
+AGS     = 0.1394118      B0      = 2.378278E-6    B1      = 5E-6
+KETA    = -8.687558E-3   A1      = 0              A2      = 1
+RDSW    = 3E3            PRWG    = -0.0286019     PRWB    = -0.0370103
+WR      = 1              WINT    = 7.514844E-7    LINT    = 1.890924E-7
+XL      = 0              XW      = 0              DWG     = -1.718509E-8
+DWB     = 3.702301E-8    VOFF    = -0.0145079     NFACTOR = 0.9590012
+CIT     = 0              CDSC    = 0              CDSCD   = 9.475364E-6
+CDSCB   = 0              ETA0    = 0.1717744      ETAB    = -0.12651
+DSUB    = 0.899852       PCLM    = 1.3374218      PDIBLC1 = 8.793855E-3
+PDIBLC2 = 2.011998E-3    PDIBLCB = -0.1           DROUT   = 0.0572504
+PSCBE1  = 1.130086E10    PSCBE2  = 2.589851E-9    PVAG    = 0.3117076
+DELTA   = 0.01           RSH     = 52.7           MOBMOD  = 1
+PRT     = 0              UTE     = -1.5           KT1     = -0.11
+KT1L    = 0              KT2     = 0.022          UA1     = 4.31E-9
+UB1     = -7.61E-18      UC1     = -5.6E-11       AT      = 3.3E4
+WL      = 0              WLN     = 1              WW      = 0
+WWN     = 1              WWL     = 0              LL      = 0
+LLN     = 1              LW      = 0              LWN     = 1
+LWL     = 0              CAPMOD  = 2              XPART   = 0.5
+CGDO    = 1.72E-10       CGSO    = 1.72E-10       CGBO    = 1E-9
+CJ      = 2.630847E-4    PB      = 0.99           MJ      = 0.5705142
+CJSW    = 1.442031E-10   PBSW    = 0.99           MJSW    = 0.1
+CJSWG   = 6.4E-11        PBSWG   = 0.99           MJSWG   = 0.1
+CF      = 0               )
*
.MODEL CMOSP PMOS (                                LEVEL   = 49
+VERSION = 3.1            TNOM    = 27             TOX     = 3.19E-8
+XJ      = 3E-7           NCH     = 2.4E16         VTH0    = -0.8476404
+K1      = 0.4513608      K2      = 2.379699E-5    K3      = 13.3278347
+K3B     = -2.2238332     W0      = 9.577236E-7    NLX     = 1E-6
+DVT0W   = 0              DVT1W   = 0              DVT2W   = 0
+DVT0    = 1.4951753      DVT1    = 0.451167       DVT2    = -0.0364224
+U0      = 236.8923827    UA      = 3.833306E-9    UB      = 1.487688E-21
+UC      = -1.08562E-10   VSAT    = 1.674377E5     A0      = 0.4435859
+AGS     = 0.1672719      B0      = 5.244897E-6    B1      = 4.525319E-6
+KETA    = 1.765523E-3    A1      = 0              A2      = 0.364
+RDSW    = 3E3            PRWG    = 0.2452639      PRWB    = -0.0635244
+WR      = 1              WINT    = 7.565065E-7    LINT    = 4.875011E-8
+XL      = 0              XW      = 0              DWG     = -2.13917E-8
+DWB     = 3.857544E-8    VOFF    = -0.0877184     NFACTOR = 0.2508342
+CIT     = 0              CDSC    = 2.924806E-5    CDSCD   = 1.497572E-4
+CDSCB   = 1.091488E-4    ETA0    = 0.26103        ETAB    = -1.34877E-3
+DSUB    = 0.2873         PCLM    = 0.0148934      PDIBLC1 = 6.876272E-4
+PDIBLC2 = 1.006023E-3    PDIBLCB = -1E-3          DROUT   = 9.918133E-4
+PSCBE1  = 3.339329E9     PSCBE2  = 5E-10          PVAG    = 14.9900194
+DELTA   = 0.01           RSH     = 76             MOBMOD  = 1
+PRT     = 0              UTE     = -1.5           KT1     = -0.11
+KT1L    = 0              KT2     = 0.022          UA1     = 4.31E-9
+UB1     = -7.61E-18      UC1     = -5.6E-11       AT      = 3.3E4
+WL      = 0              WLN     = 1              WW      = 0
+WWN     = 1              WWL     = 0              LL      = 0
+LLN     = 1              LW      = 0              LWN     = 1
+LWL     = 0              CAPMOD  = 2              XPART   = 0.5
+CGDO    = 2.13E-10       CGSO    = 2.13E-10       CGBO    = 1E-9
+CJ      = 3.004422E-4    PB      = 0.7337475      MJ      = 0.4279887
+CJSW    = 1.626626E-10   PBSW    = 0.99           MJSW    = 0.1117313
+CJSWG   = 3.9E-11        PBSWG   = 0.99           MJSWG   = 0.1117313
+CF      = 0               )
*

